;*******************************************************************
; Installation file (.inf) for the USB to Virtual Serial ports device
; VXD For WIN98
;
; (c) Copyright 2004 Ark Pioneer Microelectronics Ltd. 
;
;
; 22-Sep-2004
;*******************************************************************

[Version]
Signature="$CHICAGO$"
Provider=%ProviderName%

Class=Ports
ClassGUID={4d36e978-e325-11ce-bfc1-08002be10318}

DriverVer=06/20/2005,1.8.0.0

;--------- Manufacturer and Models Sections ----------------------------------
[Manufacturer]
%Mfg%=ArkMicro

[ArkMicro]
%DeviceDesc%=ser2up, VID_6547&PID_0232

;---------- DDInstall Sections -----------------------------------------------
; --------- Windows 98 -----------------
[ser2up]
AddReg=ser2up.AddReg
LogConfig=caa,c34,c3a,c43,c4a,c14,c1a,c23,c2a

[ser2up.AddReg]
HKR,,DevLoader,,*vcomm
HKR,,Enumerator,,serenum.vxd
HKR,,PortDriver,,ser2up.vxd
HKR,,USBDriver,,usbport.sys
HKR,,Contention,,*vcd
HKR,,ConfigDialog,,serialui.dll
HKR,,DCB,3,1C,00,00,00, 00,C2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,PortSubClass,1,01
HKR,,EnumPropPages,,"serialui.dll,EnumPropPages"

[c34]			; COM3, IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=S:4

[c3a]			; COM3, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c43]			; COM4, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=S:3,5

[c4a]			; COM4, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[caa]			; Any base, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=8@100-ffff%fff8(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c00]			; No resources
ConfigPriority=HARDRECONFIG
IOConfig=0
IRQConfig=S:000-000(000::)

[c14]			; COM1,IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=S:4

[c1a]			; COM1, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c23]			; COM2, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=S:3

[c2a]			; COM2, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

;--------- Strings Section ---------------------------------------------------

[Strings]
ProviderName="USB World Technology Inc."
Mfg="USB World"
DeviceDesc="USB Dta Cable"
DiskId = "Install disk"

